**Anexa 10 a.**

**C*ertificatului CEMT de conformitate cu cerinţele tehnice şi de siguranţă pentru autovehicule***

 ***„EURO IV/4 sigur”, „EURO V/ 5 sigur”, „EEV sigur” sau „EURO VI/ 6 sigur”***

***cu masa maximă autorizată cuprinsă între 3, 5 şi 6 tone***”.

varianta în limba engleză - **faţă**

**Certificate No: ……….**

|  |
| --- |
| **ECMT Certificate of Compliance with Technical and Safety Requirements for a Motor Vehicle (Lorry) with TPLW above 3.5 and not exceeding 6 Tonnes[[1]](#footnote-1)**❑ **"EURO IV/4 safe"** ❑ **"EURO V/5 safe"** ❑ **"EEV safe"** ❑ **"EURO VI/6 safe"** |

|  |
| --- |
| Vehicle Type and Make: |
| Vehicle Identification Number (VIN): |
| Engine Type / Number: |

The[[2]](#footnote-2)

* Competent validation Services in the country of registration,[[3]](#footnote-3)
* Vehicle Manufacturer, or the authorised Representative of the Manufacturer in the country of registration, or
* A combination of the competent validation Services in the country of registration and the vehicle Manufacturer, or the authorised Representative of the Manufacturer in the country of registration, when all the equipment is not fitted by the vehicle Manufacturer,[[4]](#footnote-4)

*[Name(s) and stamp(s) of the Company and/or the Administration]*

hereby confirms that the said vehicle is in compliance with the provisions of respective UNECE Regulations and/or EU regulatory acts, as listed below, and confirms that the particulars entered overleaf are correct.

## ENGINE POWER

❑ ❑ Measurements according to: UNECE Regulation R85.00 or as subsequently amended, or Directive 80/1269/EEC, as amended by Directive 1999/99/EC or as subsequently amended.

## REQUIREMENTS FOR NOISE AND EXHAUST EMISSIONS

❑ ❑ Noise measured according to: UNECE Regulation R51.02 or as subsequently amended, or Directive 70/157/EEC as amended by Directive 1999/101/EC or as subsequently amended.

❑ **EURO IV/4 :** Exhaust emissions according to: UNECE Regulation R49.03, row B1 or as subsequently amended, or Directive 88/77/EEC as amended by Directive 2001/27/EC, row B1 or Directive 2005/55/EC as amended by Directive 2005/78/EC, row B1 or as subsequently amended;[[5]](#footnote-5) or, exhaust emissions according to UNECE Regulation No. 83.05, row B [[6]](#footnote-6) or Directive 70/220/EEC as amended by Directive 98/69/EC, row B, and as subsequently amended by Directive 2002/80/EC.[[7]](#footnote-7)

❑ ❑ **EURO V/5 :** Exhaust emissions according to: UNECE Regulation R49.04, row B2 or as subsequently amended, or Directive 88/77/EEC as amended by Directive 2001/27/EC, row B2 or Directive 2005/55/EC as amended by Directive 2005/78/EC, row B2 or as subsequently amended [[8]](#footnote-8); or type-approval of vehicle according to UNECE Regulation No. 83.06 or Regulation (EC) No. 715/2007 as amended by Regulation (EC) No. 692/2008, or as subsequently amended. [[9]](#footnote-9)

❑ ❑ **EEV:** Exhaust emissions according to: UNECE Regulation R49.04, row Cor as subsequently amended, or Directive 88/77/EEC as amended by Directive 2001/27/EC, row C or Directive 2005/55/EC as amended by Directive 2005/78/EC, row C or as subsequently amended.[[10]](#footnote-10)

❑ ❑ **EURO VI/6 :** Type–approval of engines with respect to emissions according to: UNECE Regulation R49.06 or Regulation (EC) No 595/2009 as amended by Commission Regulation (EU) No 582/2011 and Commission Regulation (EU) No 64/2012 or as subsequently amended;[[11]](#footnote-11) or, type-approval of vehicle according to Regulation (EC) No. 715/2007 as amended by Regulation (EC) No. 692/2008, or as subsequently amended.[[12]](#footnote-12)

**C*ertificatului CEMT de conformitate cu cerinţele tehnice şi de siguranţă pentru autovehicule***

 ***„EURO IV/4 sigur”, „EURO V/ 5 sigur”, „EEV sigur” sau „EURO VI/ 6 sigur”***

***cu masa maximă autorizată cuprinsă între 3, 5 şi 6 tone***”.

varianta în limba engleză - **verso**

## SAFETY REQUIREMENTS

The motor vehicle is fitted with the following devices:

❑ ❑ **EURO IV/4 , EURO V/5  or EEV :** ***Rear protective devices[[13]](#footnote-13)*** according to UNECE Regulation R58.01 or as subsequently amended, or to Directive 70/221/EEC, as amended by Directive 2000/8/EC or as subsequently amended.

❑ ❑ **EURO VI/6 :** ***Rear protective devices*13** according to UNECE Regulation R58.02 or as subsequently amended, or to Directive 70/221/EEC as amended by Directive 2006/20/EC or as subsequently amended.

❑ ❑ ***Lateral protection*13** according to UNECE Regulation R73.00 or as subsequently amended, or to Directive 89/297/EEC or as subsequently amended.

❑ ❑ **EURO IV/4 , EURO V/5  or EEV :** ***Rear view mirror***according to UNECE Regulation R46.01 or as subsequently amended, or to Directive 71/127/EEC, as amended by Directive 88/321/EEC or Directive 2003/97/EC or as subsequently amended.

❑ ❑ **EURO VI/6 : *Indirect vision*** according to UNECE Regulation R46.02 or as subsequently amended, or to Directive 2003/97/EC or as subsequently amended.

❑ ❑ **EURO IV/4 :** ***Installation of lighting and light signaling devices*** according to UNECE Regulation R48.01 or as subsequently amended, or to Directive 76/756/EEC, as amended by Directive 91/663/EEC or as subsequently amended.

❑ ❑ **EURO V/5  or EEV :** ***Installation of lighting and light signaling devices*** according to UNECE Regulation R48.02 or as subsequently amended, or to Directive 76/756/EEC, as amended by Directive 97/28/EC or as subsequently amended.

❑ ❑ **EURO VI/6 :** ***Installation of lighting and light signaling devices*** according to UNECE Regulation R48.03 or as subsequently amended, or to Directive 76/756/EEC, as amended by Directive 2007/35/EC or as subsequently amended.

❑ ❑ **EURO IV/4 , EURO V/5  or EEV**: ***Tachograph***according to the UNECE AETR Agreement or its amendments, or to Council Regulation (EEC) No 3821/85, as amended by Regulation (EC) No 2135/98 or as subsequently amended, as well as by Commission Regulations (EC) No 1360/2002 and No 432/2004 or as subsequently amended.

❑ ❑ **EURO VI/6**: ***Digital tachograph*** according to the UNECE AETR Agreement or its amendments, or to Council Regulation (EEC) No 3821/85 as amended by Regulation (EC) No 2135/98 or as subsequently amended, as well as by Commission Regulation (EU) No 1266/2009 or as subsequently amended.

❑ ❑ ***Speed limitation devices*** according to UNECE Regulation R89.00 or as subsequently amended, or to Directive 92/24/EEC, as amended by Directive 2004/11/EC or as subsequently amended.

❑ ❑ **EURO IV/4 , EURO V/5 or EEV**: ***Braking, including antiblocking systems*** according to UNECE Regulation R13.09 or as subsequently amended, or to Directive 71/320/EEC as amended by Directive 98/12/EC or as subsequently amended.

❑ ❑ **EURO VI/6**: ***Braking, including antiblocking systems*** according to UNECE Regulation R13.10 or as subsequently amended, or to Directive 71/320/EEC, as amended by Directive 2002/78/EC or as subsequently amended.

❑ ❑ ***Steering*** according to UNECE Regulation R79.01 or as subsequently amended, or to Directive 70/311/EEC as amended by Directive 1999/7/EC or as subsequently amended.

Place Date Signature(s) and stamp(s) [[14]](#footnote-14)

1. . Lorries above 6 tonnes type approved according to light duty vehicle emissions regulations or equipped with petrol engines are included. [↑](#footnote-ref-1)
2. . Delete inappropriate mentions. [↑](#footnote-ref-2)
3. . For the countries where the Representatives of the manufacturers are not authorised. [↑](#footnote-ref-3)
4. . In this case, the first Signatory fills in the column on the left, the second Signatory fills in the column on the right. [↑](#footnote-ref-4)
5. . Character B1 or B or C, in the approval number. [↑](#footnote-ref-5)
6. . Character II in the approval number. [↑](#footnote-ref-6)
7. . Character B in the approval number. [↑](#footnote-ref-7)
8. . Character B2 or D, E, F or G, in the approval number. [↑](#footnote-ref-8)
9. . Characters A to M in the approval number. [↑](#footnote-ref-9)
10. . Character C or H, I, J or K in the approval number. [↑](#footnote-ref-10)
11. . Character A, B or C in the approval number. [↑](#footnote-ref-11)
12. . Characters N to ZC in the approval number. [↑](#footnote-ref-12)
13. . Semi-trailer tractor excepted. [↑](#footnote-ref-13)
14. . Certificate may be filled in, stamped and signed manually or electronically. [↑](#footnote-ref-14)