**Anexa 10.b.**

***certificatul de conformitate cu cerinţele tehnice de siguranţă pentru remorca cu masa maxima autorizată care nu depăşeşte 3,5 tone;***

varianta în limba engleză

**Certificate No: ..................**

**ECMT Certificate of Compliance of a Trailer of TPLW not exceeding 3.5 Tonnes [[1]](#footnote-1) with the Technical Safety Requirements**

|  |
| --- |
| Vehicle Type and Make: |
| Vehicle Identification Number (VIN): |

The[[2]](#footnote-2)

-- Competent validation Services in the country of registration,[[3]](#footnote-3)

-- Vehicle Manufacturer, or the authorised Representative of the Manufacturer in the country of registration, or

-- A combination of the competent validation Services in the country of registration and the vehicle Manufacturer, or the authorised Representative of the Manufacturer in the country of registration, when all the equipment is not fitted by the vehicle Manufacturer,[[4]](#footnote-4)

*[Name(s) of the Company and/or the Administration]*

hereby confirms that the said vehicle is in compliance with the provisions of respective UN Regulations and/or EC Directives, as listed below, and confirms that the particulars entered overleaf are correct.

The trailer is fitted with the following devices:

❑ ❑ Rear underrun protective devices according to UN Regulation No. 58.01 or as subsequently amended; or to Directive 70/221/EEC, as amended by Directive 2000/8/EC or as subsequently amended.

❑ ❑ Installation of lighting and light signaling devices according to UN Regulation No. 48.01 or as subsequently amended; or to Directive 76/756/EEC, as amended by Directive 91/663/EEC, or as subsequently amended.

❑ ❑ Braking[[5]](#footnote-5) according to UN Regulation No. 13.09 or as subsequently amended; or to Directive 71/320/EEC, as amended by Directive 98/12/EC, or as subsequently amended.

❑ ❑ Mechanical couplings according to UN Regulation No. 55.01 or to Directive 94/20/EC, including secondary coupling device (if applicable).

Place Date Signature(s) and stamp(s)[[6]](#footnote-6)

1. . Semi-trailers included. [↑](#footnote-ref-1)
2. . Delete inappropriate mentions. [↑](#footnote-ref-2)
3. . For the countries where the Representatives of the manufacturers are not authorised. [↑](#footnote-ref-3)
4. . In this case, the first signatory fills in the column on the left, the second signatory fills in the column on the right. [↑](#footnote-ref-4)
5. . For O1 is not mandatory. [↑](#footnote-ref-5)
6. . Certificate may be filled in, stamped and signed manually or electronically. [↑](#footnote-ref-6)