**Anexa 9.b.**

**Modelul certificatului CEMT de conformitate cu normele tehnice de siguranță pentru remorci/semiremorci; *varianta în limba engleză;***

**Certificate No: ..................**

**ECMT Certificate of Compliance of a Trailer[[1]](#footnote-1) with the Technical Safety Requirements**

|  |
| --- |
| Vehicle Type and Make: |
| Vehicle Identification Number (VIN): |

The[[2]](#footnote-2)

-- Competent validation Services in the country of registration,[[3]](#footnote-3)

-- Vehicle Manufacturer, or the authorised Representative of the Manufacturer in the country of registration, or

-- A combination of the competent validation Services in the country of registration and the vehicle Manufacturer, or the authorised Representative of the Manufacturer in the country of registration, when all the equipment is not fitted by the vehicle Manufacturer,[[4]](#footnote-4)

*[Name(s) of the Company and/or the Administration]*

hereby confirms that the said vehicle is in compliance with the provisions of respective UN Regulations and/or EC Directives, as listed below, and confirms that the particulars entered overleaf are correct.

The trailer is fitted with the following devices:

❑ ❑ Rear underrun protective devices according to UN Regulation No. 58.01 or as subsequently amended; or to Directive 70/221/EEC, as amended by Directive 2000/8/EC or as subsequently amended.

❑ ❑ Lateral protection according to UN Regulation No. 73.00 or as subsequently amended; or to Directive 89/297/EEC or as subsequently amended.

❑ ❑ Lighting and light-signalling devices according to UN Regulation No. 48.02 or as subsequently amended; or to Directive 76/756/EEC, as amended by Directive 91/663/EEC, or as subsequently amended.

❑ ❑ Rear marking plates (retroreflective) for heavy and long vehicles according to UN Regulation No. 70.01 or as subsequently amended.[[5]](#footnote-5)

❑ ❑ Braking, including anti-lock braking systems, according to UN Regulation No. 13.10 or as subsequently amended; or to Directive 71/320/EEC, as amended by Directive 98/12/EC, or as subsequently amended.

Place Date Signature(s) and stamp(s)[[6]](#footnote-6)

1. . Semi-trailers included. [↑](#footnote-ref-1)
2. . Delete inappropriate mentions. [↑](#footnote-ref-2)
3. . For the countries where the Representatives of the manufacturers are not authorised. [↑](#footnote-ref-3)
4. . In this case, the first signatory fills in the column on the left, the second signatory fills in the column on the right. [↑](#footnote-ref-4)
5. . Or, conspicuity marking according to UN Regulation No. 48.03 or as subsequently amended. [↑](#footnote-ref-5)
6. . Certificate may be filled in, stamped and signed manually or electronically. [↑](#footnote-ref-6)